A white truck with a small white box on it

AI-generated content may be incorrect.

**HALF CABIN AMBULIFT HCATLZ 4500**

**CAPACITY: 2000 kg**

**OPERATIVE RANGE: 1600/4500 mm**

Ambulift on ISUZU P75-K (or on request a similar IVECO vehicle), has been designed for the transport of disabled people in wheelchairs and on stretchers sick from ground level.

**HALF CABIN AMBULIFT HCATLZ1645**

A drawing of a trailer

AI-generated content may be incorrect.

A drawing of a cart

AI-generated content may be incorrect.

|  |  |  |
| --- | --- | --- |
| **TECHNICAL SPECIFICATION** | | |
| Truck: Isuzu P75-K  Wheelbase 3815 mm  Overall width 2500mm  Height 3975 mm  Total Length 6500 mm | Minimum height from ground (with stabilizer feet) 1600 mm Maximum height from ground (with stabilizer feet) 4500 mm Operating speed max 30 Km/h  Max wind speed 74 Km/h | |
| **Sizes vanbody (external)** | **Sizes of the platforms** | |
| Width 2450 mm | **Front** | **Rear** |
|  |  |
| Height(without air cond. system) 2330 mm | Width 900 mm | Width 2200 mm |
| Length 4500 mm | Length 1650 mm | Length 1700 mm |
| Capacity Vanload 2000 Kg  (6 passengers in wheelchairs and 2 assistants, or 2 stretchers and 4 passengers in wheelchairs and 2 assistants, or 10 people standing and 2 assistants) | Longitudinal movement 500 mm Working height 1600 mm  Capacity 454 Kg | Working height to floor 0-1600mm Capacity 700 Kg |