

**HALF CABIN AMBULIFT HCTLZ5800**

**CAPACITY: 2000 kg OPERATIVE RANGE: 1650/5800 mm**

Ambulift on ISUZU F14NQ (or on request a similar IVECO vehicle), has been designed for the transport of disabled people in wheelchairs and on stretchers sick from ground level.

**HALF CABIN AMBULIFT HCTLZ5800**





|  |
| --- |
| **TECHNICAL SPECIFICATION** |
| Truck ISUZU F14NQWheelbase 5320 mmOverall width 2500mmHeight 4090 mmTotal Length 8900 mm | Minimum height from ground (with stabilizer feet) 1650 mm Maximum height from ground (with stabilizer feet) 5800 mm Operating speed max 30 Km/hMax wind speed 74 Km/h |
| **Sizes vanbody (external)** | **Sizes of the platforms** |
| Width 2290 mmHeight(without air cond. system) 2270 mm Length 6900 mmCapacity Vanload 2000 Kg(9 passengers in wheelchairs and 2 assistants, or 4 stretchers and 2 assistants) | **Front** | **Rear** |
| Width 850 mmLength 1800 mmLongitudinal movement 500 mm Working height 1650 mmCapacity 454 Kg | Width 2200 mmLength 1700 mmWorking height to floor 0-1600mm Capacity 700 Kg |