A large white truck with a lift

AI-generated content may be incorrect.

**HALF CABIN AMBULIFT HCTLZ5800**

**CAPACITY: 2000 kg OPERATIVE RANGE: 1650/5800 mm**

Ambulift on ISUZU F14NQ (or on request a similar IVECO vehicle), has been designed for the transport of disabled people in wheelchairs and on stretchers sick from ground level.

**HALF CABIN AMBULIFT HCTLZ5800**

A drawing of a trailer

AI-generated content may be incorrect.

A drawing of a cart

AI-generated content may be incorrect.

|  |  |  |
| --- | --- | --- |
| **TECHNICAL SPECIFICATION** | | |
| Truck ISUZU F14NQ  Wheelbase 5320 mm  Overall width 2500mm  Height 4090 mm  Total Length 8900 mm | Minimum height from ground (with stabilizer feet) 1650 mm Maximum height from ground (with stabilizer feet) 5800 mm Operating speed max 30 Km/h  Max wind speed 74 Km/h | |
| **Sizes vanbody (external)** | **Sizes of the platforms** | |
| Width 2290 mm  Height(without air cond. system) 2270 mm Length 6900 mm  Capacity Vanload 2000 Kg  (9 passengers in wheelchairs and 2 assistants, or 4 stretchers and 2 assistants) | **Front** | **Rear** |
| Width 850 mm  Length 1800 mm  Longitudinal movement 500 mm Working height 1650 mm  Capacity 454 Kg | Width 2200 mm  Length 1700 mm  Working height to floor 0-1600mm Capacity 700 Kg |